**Integrating PPA into a new NPI**

Introduction :

PPA (Primary Protected Application) binary can be integrated into a new NPI using the following commands in the respective command prompt shells.

**:: Simulator ::**

top.ccm.mem.real.write\_from\_file(0x20A00000, PATH+"ppa.itb")

**:: PXP ::**

memory -load %pd\_raw2 -file $TEST\_PATH/ppa.itb $memory -start 0xA00000

**:: CFP ::**

[CFP Shell] # ./cfp -m 0x9B000000 -f /home/root/v42/sudhanshu/ls1028\_binaries/ppa.itb